(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "DFE201610P-1R0M=P2" (in_bom yes) (on_board yes) (pin_names hide)
    (property "Reference" "L" (at 16.51 6.35 0))
    (property "Value" "DFE201610P-1R0M=P2" (at 16.51 3.81 0))
    (property "Footprint" "1285ASH1R0MP2" (at 16.51 -96.19 0))
    (property "Datasheet" "https://psearch.en.murata.com/inductor/product/DFE201610P-1R0M%23.html" (at 16.51 -196.19 0))
    (property "ki_description" "Toko DFE201610P Series Shielded Wire-wound SMD Inductor with a Powered Iron Core, 1 uH Wire-Wound 3.4A Idc" (at 16.51 -296.19 0))
    (property "Height" "1" (at 16.51 -396.19 0))
    (property "Mouser Part Number" "81-DFE201610P-1R0MP2" (at 16.51 -496.19 0))
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/DFE201610P-1R0M%3dP2?qs=KuGPmAKtFKXuKbjOYjhb2A%3D%3D" (at 16.51 -596.19 0))
    (property "Manufacturer_Name" "Murata Electronics" (at 16.51 -696.19 0))
    (property "Manufacturer_Part_Number" "DFE201610P-1R0M=P2" (at 16.51 -796.19 0))
    (pin passive line (at 0 0 0) (length 5.08)
      (name "1")
      (number "1")
    )
    (pin passive line (at 20.32 0 180) (length 5.08)
      (name "2")
      (number "2")
    )
  )
)
