(kicad_pcb (version 4) (host pcbnew "(2015-10-23 BZR 6276, Git f0eaafc)-product")
  (general
    (links 120)
    (no_connects 0)
    (area 79.570143 35.651 173.977286 73.546)
    (thickness 1.6)
    (drawings 23)
    (tracks 765)
    (zones 0)
    (modules 24)
    (nets 61)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.9 1.9)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory fab/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 p2_g1)
  (net 4 p2_b1)
  (net 5 strobe)
  (net 6 p2_r1)
  (net 7 p2_r2)
  (net 8 p0_r1)
  (net 9 p0_g1)
  (net 10 OE)
  (net 11 p0_b1)
  (net 12 p0_r2)
  (net 13 p0_g2)
  (net 14 row_D)
  (net 15 row_C)
  (net 16 p0_b2)
  (net 17 clock)
  (net 18 row_B)
  (net 19 row_A)
  (net 20 p1_g1)
  (net 21 p1_b1)
  (net 22 p1_r1)
  (net 23 p1_g2)
  (net 24 p1_r2)
  (net 25 p2_g2)
  (net 26 p1_b2)
  (net 27 p2_b2)
  (net 28 p0_r1_buff)
  (net 29 p0_g1_buff)
  (net 30 p0_b1_buff)
  (net 31 p0_r2_buff)
  (net 32 p0_g2_buff)
  (net 33 p0_b2_buff)
  (net 34 row_A_buff)
  (net 35 row_B_buff)
  (net 36 row_C_buff)
  (net 37 row_D_buff)
  (net 38 clock_buff_0)
  (net 39 strobe_buff_0)
  (net 40 OE_buff_0)
  (net 41 p1_r1_buff)
  (net 42 p1_g1_buff)
  (net 43 p1_b1_buff)
  (net 44 p1_r2_buff)
  (net 45 p1_g2_buf)
  (net 46 p1_b2_buff)
  (net 47 clock_buff_1)
  (net 48 strobe_buff_1)
  (net 49 OE_buff_1)
  (net 50 p2_r1_buff)
  (net 51 p2_g1_buff)
  (net 52 p2_b1_buff)
  (net 53 p2_r2_buff)
  (net 54 p2_g2_buf)
  (net 55 p2_b2_buff)
  (net 56 clock_buff_2)
  (net 57 strobe_buff_2)
  (net 58 OE_buff_2)
  (net 59 "Net-(P1-Pad1)")
  (net 60 "Net-(P1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net OE)
    (add_net OE_buff_0)
    (add_net OE_buff_1)
    (add_net OE_buff_2)
    (add_net clock)
    (add_net clock_buff_0)
    (add_net clock_buff_1)
    (add_net clock_buff_2)
    (add_net p0_b1)
    (add_net p0_b1_buff)
    (add_net p0_b2)
    (add_net p0_b2_buff)
    (add_net p0_g1)
    (add_net p0_g1_buff)
    (add_net p0_g2)
    (add_net p0_g2_buff)
    (add_net p0_r1)
    (add_net p0_r1_buff)
    (add_net p0_r2)
    (add_net p0_r2_buff)
    (add_net p1_b1)
    (add_net p1_b1_buff)
    (add_net p1_b2)
    (add_net p1_b2_buff)
    (add_net p1_g1)
    (add_net p1_g1_buff)
    (add_net p1_g2)
    (add_net p1_g2_buf)
    (add_net p1_r1)
    (add_net p1_r1_buff)
    (add_net p1_r2)
    (add_net p1_r2_buff)
    (add_net p2_b1)
    (add_net p2_b1_buff)
    (add_net p2_b2)
    (add_net p2_b2_buff)
    (add_net p2_g1)
    (add_net p2_g1_buff)
    (add_net p2_g2)
    (add_net p2_g2_buf)
    (add_net p2_r1)
    (add_net p2_r1_buff)
    (add_net p2_r2)
    (add_net p2_r2_buff)
    (add_net row_A)
    (add_net row_A_buff)
    (add_net row_B)
    (add_net row_B_buff)
    (add_net row_C)
    (add_net row_C_buff)
    (add_net row_D)
    (add_net row_D_buff)
    (add_net strobe)
    (add_net strobe_buff_0)
    (add_net strobe_buff_1)
    (add_net strobe_buff_2)
  )
  (net_class power ""
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 562B1C37)
    (at 106.172 57.912 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -3.088 0.578 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 557C6230)
    (at 123.952 57.912 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.162 0.548 90) (layer F.SilkS))
    (fp_text value 100n (at -0.338 1.798 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 557C623A)
    (at 141.732 57.912 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.088 0.018 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 557C6244)
    (at 159.512 57.912 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.588 1.988 180) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 (layer F.Cu) (tedit 562B1708)
    (at 107.95 43.18 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 3.302 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_02X20 (at 0 -3.1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 p2_g1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 p2_b1))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 strobe))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 p2_r1))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 clock))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 OE))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 p0_g1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 row_A))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 row_B))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 row_C))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 p0_b2))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 p0_g2))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 row_D))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 p0_r1))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 p0_r2))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 p0_b1))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 p1_g1))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 p1_b1))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 p1_r1))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 p1_g2))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 p1_r2))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 p2_g2))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 p2_r2))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 p1_b2))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 p2_b2))
    (model Pin_Headers/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08 (layer F.Cu) (tedit 562BDA69)
    (at 88.9 67.056 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Panel-1 (at 1.905 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 0 -3.1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 p0_r1_buff))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 p0_g1_buff))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 p0_b1_buff))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 p0_r2_buff))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 p0_g2_buff))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 p0_b2_buff))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 row_A_buff))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 row_B_buff))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 row_C_buff))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 row_D_buff))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 clock_buff_0))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 strobe_buff_0))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 OE_buff_0))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08 (layer F.Cu) (tedit 54F3ABF0)
    (at 116.84 67.056 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Panel-2 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 0 -3.1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 p1_r1_buff))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 p1_g1_buff))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 p1_b1_buff))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 p1_r2_buff))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 p1_g2_buf))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 p1_b2_buff))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 row_A_buff))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 row_B_buff))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 row_C_buff))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 row_D_buff))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 clock_buff_1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 strobe_buff_1))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 OE_buff_1))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x08 (layer F.Cu) (tedit 54F3ABEC)
    (at 144.78 67.056 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference Panel-3 (at 1.27 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_02X08 (at 0 -3.1 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 p2_r1_buff))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 p2_g1_buff))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 p2_b1_buff))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 p2_r2_buff))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 p2_g2_buf))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 p2_b2_buff))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 row_A_buff))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 row_B_buff))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 row_C_buff))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 row_D_buff))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 clock_buff_2))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 strobe_buff_2))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 OE_buff_2))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x08.wrl
      (at (xyz 0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:1pin locked (layer F.Cu) (tedit 562B1509)
    (at 103.08 41.91)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P20 (at 0.044 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:1pin locked (layer F.Cu) (tedit 562B1502)
    (at 161.08 41.91)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P21 (at -0.044 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 562B1CC5)
    (at 97.79 54.356 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -7.5 270) (layer F.SilkS))
    (fp_text value 74HCT245 (at -2.032 -2.794 360) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 OE))
    (pad 3 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 clock))
    (pad 4 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 p0_b2))
    (pad 5 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 p0_r2))
    (pad 6 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 p0_g2))
    (pad 7 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 p0_b1))
    (pad 8 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 p0_r1))
    (pad 9 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 p0_g1))
    (pad 10 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 p0_g1_buff))
    (pad 12 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 p0_r1_buff))
    (pad 13 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 p0_b1_buff))
    (pad 14 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 p0_g2_buff))
    (pad 15 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 p0_r2_buff))
    (pad 16 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 p0_b2_buff))
    (pad 17 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 clock_buff_0))
    (pad 18 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 OE_buff_0))
    (pad 19 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 562B1CBB)
    (at 115.57 54.356 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -7.5 270) (layer F.SilkS))
    (fp_text value 74HCT245 (at -1.778 -2.54 360) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 strobe))
    (pad 4 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 strobe))
    (pad 5 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 row_D))
    (pad 6 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 row_C))
    (pad 7 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 row_A))
    (pad 8 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 row_B))
    (pad 9 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 strobe))
    (pad 10 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 strobe_buff_0))
    (pad 12 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 row_B_buff))
    (pad 13 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 row_A_buff))
    (pad 14 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 row_C_buff))
    (pad 15 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 row_D_buff))
    (pad 16 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 strobe_buff_1))
    (pad 17 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 strobe_buff_2))
    (pad 18 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 562B1CB7)
    (at 133.35 54.356 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 270) (layer F.SilkS))
    (fp_text value 74HCT245 (at -1.778 -2.286 360) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 OE))
    (pad 3 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 clock))
    (pad 4 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 p1_b2))
    (pad 5 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 p1_r2))
    (pad 6 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 p1_g2))
    (pad 7 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 p1_b1))
    (pad 8 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 p1_r1))
    (pad 9 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 p1_g1))
    (pad 10 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 p1_g1_buff))
    (pad 12 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 p1_r1_buff))
    (pad 13 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 p1_b1_buff))
    (pad 14 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 p1_g2_buf))
    (pad 15 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 p1_r2_buff))
    (pad 16 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 p1_b2_buff))
    (pad 17 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 clock_buff_1))
    (pad 18 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 OE_buff_1))
    (pad 19 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 562B1CC1)
    (at 151.13 54.356 270)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 -7.5 270) (layer F.SilkS))
    (fp_text value 74HCT245 (at -1.778 -2.286 360) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 OE))
    (pad 3 smd rect (at -4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 clock))
    (pad 4 smd rect (at -4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 p2_b2))
    (pad 5 smd rect (at -4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 p2_r2))
    (pad 6 smd rect (at -4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 p2_g2))
    (pad 7 smd rect (at -4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 p2_b1))
    (pad 8 smd rect (at -4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 p2_r1))
    (pad 9 smd rect (at -4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 p2_g1))
    (pad 10 smd rect (at -4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 p2_g1_buff))
    (pad 12 smd rect (at 4.7 4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 p2_r1_buff))
    (pad 13 smd rect (at 4.7 3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 p2_b1_buff))
    (pad 14 smd rect (at 4.7 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 p2_g2_buf))
    (pad 15 smd rect (at 4.7 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 p2_r2_buff))
    (pad 16 smd rect (at 4.7 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 p2_b2_buff))
    (pad 17 smd rect (at 4.7 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 clock_buff_2))
    (pad 18 smd rect (at 4.7 -3.175 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 OE_buff_2))
    (pad 19 smd rect (at 4.7 -4.445 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 562BCA64)
    (at 105.664 46.736)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.556 0) (layer F.SilkS))
    (fp_text value 10k (at -0.762 -1.778) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 OE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 562BC84E)
    (at 92.71 42.799 90)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at 5.08 -1.397 180) (layer F.SilkS))
    (fp_text value 22u (at 1.25 4.4 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 562BCBDD)
    (at 119.38 45.847 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value RxD (at -3.81 -0.127 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P1-Pad10)"))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 562B2A82)
    (at 87.376 41.783 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 4.064 -0.254 180) (layer F.SilkS))
    (fp_text value 22u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 562B353C)
    (at 87.376 49.022 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -2.286 0 180) (layer F.SilkS) hide)
    (fp_text value +5V (at 1.778 -5.334 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.54 3.048) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 562B354A)
    (at 87.376 54.102 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0.254 2.54 90) (layer F.SilkS) hide)
    (fp_text value GND (at 0.254 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.54 3.048) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 562BCBF7)
    (at 110.744 45.847 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value GND (at -3.937 -0.127 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.9 1.9) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop locked (layer F.Cu) (tedit 562BD77F)
    (at 164 39)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value TopRight (at 6.434 -2.17) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop locked (layer F.Cu) (tedit 562BD774)
    (at 86 70)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at -3.958 0.739) (layer F.SilkS) hide)
    (fp_text value BottomLeft (at -0.402 2.517) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen locked (layer F.Cu) (tedit 562BD9C4)
    (at 162.814 50.165)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 6.477 -3.175) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 5.461 5.461 90) (layer F.Fab) hide)
  )
  (gr_text "RPi Power IN\n" (at 90.297 51.816 270) (layer F.SilkS))
  (gr_text "GND\n" (at 85.598 58.166 270) (layer F.SilkS))
  (gr_text +5V (at 85.598 44.958 270) (layer F.SilkS))
  (gr_text 1 (at 144.78 70.358) (layer F.SilkS))
  (gr_text 1 (at 116.84 70.358) (layer F.SilkS))
  (gr_text 1 (at 88.9 70.358) (layer F.SilkS))
  (gr_text 1 (at 105.156 49.022 180) (layer F.SilkS))
  (gr_text 1 (at 158.496 49.022 180) (layer F.SilkS))
  (gr_text 1 (at 140.716 49.022 180) (layer F.SilkS))
  (gr_text %%gitversion%% (at 135.636 51.816) (layer B.SilkS))
  (gr_text 1 (at 122.936 49.022 180) (layer F.SilkS))
  (gr_text github.com/hzeller/rpi-rgb-led-matrix (at 128.016 37.846) (layer F.SilkS))
  (gr_text "USB-ports ->" (at 165.1 45.72) (layer F.SilkS))
  (gr_text "Bottom Chain (3)\n" (at 153.67 60.96) (layer F.SilkS))
  (gr_text "Middle Chain (2)" (at 126.492 60.96) (layer F.SilkS))
  (gr_text "Top Chain (1)" (at 97.79 60.96) (layer F.SilkS))
  (gr_line (start 84 71.5) (end 84 36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84 36) (end 167 36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167 36) (end 167 71.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167 71.5) (end 84 71.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.75 71.25) (xy 84.25 71.25) (xy 84.25 36.25) (xy 166.75 36.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.25 36.25) (xy 166.75 36.25) (xy 166.75 71.25) (xy 84.25 71.25)
      )
    )
  )
)
