(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BQ24210DQCR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 11.43 0)
		)
		(property "Value" "BQ24210DQCR"
			(at 0 -11.43 0)
		)
		(property "Footprint" "lib:WSON-10_L3.0-W2.0-P0.50-BL-EP"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://lcsc.com/product-detail/PMIC-Battery-Management_Texas-Instruments-Texas-Instruments-BQ24210DQCR_C524795.html"
			(at 0 -16.51 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "LCSC Part" "C524795"
			(at 0 -19.05 0)
		)
		(symbol "BQ24210DQCR_0_1"
			(pin unspecified line
				(at -11.43 3.81 0)
				(length 2.54)
				(name "VBUS")
				(number "1")
			)
			(pin unspecified line
				(at -11.43 1.27 0)
				(length 2.54)
				(name "ISET")
				(number "2")
			)
			(pin unspecified line
				(at -11.43 -1.27 0)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin unspecified line
				(at -11.43 -3.81 0)
				(length 2.54)
				(name "VTSB")
				(number "4")
			)
			(pin unspecified line
				(at -11.43 -6.35 0)
				(length 2.54)
				(name "TS")
				(number "5")
			)
			(pin unspecified line
				(at 11.43 6.35 180)
				(length 2.54)
				(name "EP")
				(number "11")
			)
			(pin unspecified line
				(at 11.43 3.81 180)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin unspecified line
				(at 11.43 1.27 180)
				(length 2.54)
				(name "VDPM")
				(number "9")
			)
			(pin unspecified line
				(at 11.43 -1.27 180)
				(length 2.54)
				(name "~{CHG}")
				(number "8")
			)
			(pin unspecified line
				(at 11.43 -3.81 180)
				(length 2.54)
				(name "~{EN}")
				(number "7")
			)
			(pin unspecified line
				(at 11.43 -6.35 180)
				(length 2.54)
				(name "~{PG}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
)
